Wirral Slot Car Club

  Address: Vale Park, The Coach House, Magazine Ln, Wallasey CH45 1LZ. Phone: 07751 899481
POLICAR CLASSIC F1 2024 
6th April 


Policar GP Event Format

Saturday
9am – Free Practice
Midday - Standard Class Heats followed by Standard Class ‘step up’ Finals.

Racing Format
Every entrant will get four 3 minute Heats, one on each Lane.
The best 2 runs will count for your qualifying position in the step up Finals.
The Finals will be over a fixed number of Laps on a single lane.
Top Qualifier in each Final gets 1st choice of Lane.
The winner of each Final will step up to the next one (depending on the entry on the day we may alter this to the top 2 to step up).
Car Rules reminders; 
Standard Class
Cars must be as manufactured with only the following changes permitted.
Policar replacement aluminium rear wheels may be fitted (correct inserts are required).
Policar F22 or G25 replacement Rear Tyres may be fitted. These may be glued, trued and treated but must be dry whenever the car is placed on the track.
Width over the rear wheels must not exceed 65mm.
Front tyres may be glued and trued and may be coated.
Weight may be added inside the car only.
Braids and lead wire are free choice.
Body and Pod Screws may be run loose, but please ensure that they cannot fall out.
Minor scraping and sanding of the Body, Chassis and Pod is allowed to obtain free movement of these parts.
Eligible Cars.
Lotus 72
March 701
Ferrari 312B2
BRM P160 & P153

The Ferrari 126C2 IS NOT eligible for the standard class.
Liveries.
Cars may race in the original Policar liveries or may be repainted if desired.
Any repaints/white kits must be painted in a genuine livery as used on the real car in a Formula 1 race.

Body shell.
Must be original Policar, be as complete as possible and include suspension detail etc.
Body shells may be modified to represent alternative versions of the car at other races.
Front and Rear wings must be securely attached to the car at the start of every race.
Parts may be glued in place as desired.
(We understand that small parts, such as mirrors, can get knocked of during practice and racing and will not insist on these items being replaced during the event).

Chassis & Motor pod.
These items must be genuine Policar parts and must not be modified or have parts removed. MINOR scraping or sanding of the chassis/motor pod edges, to allow for body float, will be allowed.
Chassis and body screws may be loose or removed as desired but please ensure that any loose screws cannot fall out during races.
All screws are free choice.
Grub screws may be fitted in the holes provided at the front of the chassis to set the front axle height.
Motor.
Must be an original Policar FF050 slim can motor of the same specification as that supplied with the car. Part no’s PMX01 or PMX01-k.



Gears & Rear Axle.
All gears and the rear axle must be genuine Policar parts to the same specification as supplied with the car.
Only the standard 17 tooth final drive gear/rear axle may be used, the optional final drive gear ratios may not be used for the standard class.
Wheels & Tyres.
Front wheels must be the original Poilcar plastic wheels – Part no PW13807921P.
Front tyres must be original Policar tyres.
a. Treaded tyres – Part no PPT1220C1
b. Slick tyres – Part no PPT1354C1.
Front track width must remain standard.
Front tyres may be glued and trued if desired.
Coating of the front tyres is permitted for the standard class.
Rear wheels must be one of the following:
1. The original Policar plastic wheels as supplied with the car;
a. Part no PW16011724P – 16mm wheels.
b. Part no PW13813519P – 13.8mm wheels.
2. Policar Aluminium Wheels;
a. Part no PW16011724A – for the early cars with 16mm wheels
b. Part no PW13813519A – for the later cars with 13.8mm whee
Rear tyres must be one of the following:
1. The original Policar tyres as supplied with the car.
a. Treaded tyres – Part no PPT1219C1 for 16mm wheels.
b. Slick tyres – Part no PPT1370C1 for 16mm wheels.
c. Slick tyres – Part no PPT1224C1 for 13.8mm wheels.
2. Policar F22 slicks – Part no PPT1219F22 for 16mm wheels.
3. Policar G25 slicks
a. Part no PPT1310G25 for 16mm wheels
b. Part no PPT1224G25 for 13.8mm wheels.
Overall width measured over the rear wheels and tyres must not exceed 65mm.
Rear tyres may be glued and trued if desired.
Rear tyres must be dry whenever the car is placed on the track and any cleaning fluid / treatment used on the tyres must not leave any residue on the track.
All Wheels must have the correct inserts for the car fitted.


Guide.
Must be a genuine Policar guide to the same specification as supplied with any of the eligible cars. Braids & Lead Wire are free choice.


Additional Weight.
Weight may be added inside the car only.
No weight will be allowed underneath the chassis and any added weight must not be visible outside the car.
	
	Details 
	Programme.

	Entrant Costs 
	£10 
	Food will be supplied. 

	Start (doors open ) 
	0900am 
	Race start 1pm 

	Awards for the top finishers with a special award for the best guest racer 
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